Specifications

Models

SETU ATA1S VoIP Adaptor with 1 FXS Port

SETU ATA2S VoIP Adaptor with 2 FXS Ports

Parameters

SETU ATA1S and SETU ATA2S

VoIP

Protocol SIPv2, SDP, RTP (RFC 2833)

Network Protocol IPv4, TCP, UDP, PPPoE, DHCP Server & Client, SNTP, NAT, STUN, HTTP, PPP, Dynamic DNS, Port Forwarding and DMZ

Connector Ethernet (RJ45)

SIP Accounts 3

Voice Codecs G.711 (A/µ Law), G.723, G.729AB, GSM-FR, GSM-EFR and iLBC

Fax over IP (FoIP) T.38 and Pass-Through

Security SRTP/TLS over SIP

FXS

Connector RJ11

Dialing and Reception DTMF and FSK CLI Presentation

Answering and Disconnect Signaling Polarity Reversal for call connect/disconnect signaling

Power Supply

External Power Adaptor 12VDC, 1.25A

Power Consumption 5W (Typical)

Other

Dimensions (WxHxD) 7.9 x 10.5 x 2.7cms (3.1”x 4.1”x 1.1”)

Weight 0.45 Kgs (1.10 lbs)

Mounting Options Wall Mount and Table Top

Operating Temperature -10°C to +50°C (-14°F to +122°F)